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Industrial environmental monitoring (IEM) in “Surgutneftegas” PJSC is performed on the basis of GOST R 56059-2014 “Industrial environmental monitoring. General provisions” to provide information on the environment condition and pollution level required to perform activity on preservation and restoration of the natural environment, rational use and reproduction of natural resources, prevention of the negative impact of business and other activity on the environment and elimination of its consequences.
According to GOST R 56059-2014, environmental analytical measurement can be performed only by in-house or third-party laboratories that are accredited for required measuring in compliance with the current legislation of the Russian Federation and have license to operate in the sphere of hydrometeorology and related areas.
“Surgutneftegas” PJSC has license No. L039-00117-77/00299159 dated 17.06.2022 to operate in the sphere of hydrometeorology and related areas, including determination of the pollution level of ambient air, soils and water bodies.
In the territory of the Republic of Sakha (Yakutia), environmental monitoring within subsoil plots is performed in compliance with the developed and approved environmental monitoring programs. 
In 2025, environmental monitoring was performed at 21 subsoil plots of “Surgutneftegas” PJSC in the territory of the Republic of Sakha (Yakutia), including local environmental monitoring (hereinafter – LEM) at 110 sampling points at six subsoil plots, and monitoring in the area of waste disposal facilities (sludge pits) at all 18 subsoil plots. 
This report presents the results of LEM of the territories of the Talakansky, Alinsky, Severo-Talakansky, Vostochno-Talakansky, Vostochno-Alinsky and Yuzhno-Talakansky subsoil plots.
During organization of monitoring, the regional features were taken into consideration: developed river net, existence of temporary (drying up with the seasonal runoff) brooks, which appear mainly during the spring flooding, open and closed lakes with marshlands in bottom-lands of the small rivers and brooks, the results of evaluation of the current background pollution of the plot, as well as the location of the production facilities. Monitoring points are installed at major water bodies of subsoil plots, at the prevailing types of soils as well as the areas where the Company’s production facilities are placed that pose potential environmental risks. All points are fixed in the field by identification marks containing information about number, geographical coordinates and name of the subsoil plot.
Monitoring points network is divided into two groups:
- baseline monitoring points located outside the zone of the direct impact of man-made facilities;
- monitoring checkpoints located in the areas of potential sources of a man-made impact.
Natural environment components under study: surface waters, bottom sediments, soils, ambient air, and snow cover.
Table 1. The structure of the observational network of local environmental monitoring within subsoil plots of “Surgutneftegas” PJSC in the Republic of Sakha (Yakutia)
	Natural environment
components
	Number of points
	Number of controlled parameters

	
	Baseline
	Control
	

	Ambient air
	6
	10
	5

	Surface waters
	12
	27
	21

	Bottom sediments
	10
	25
	13

	Soils
	6
	10
	25

	Snow cover
	2
	10
	13


The laboratory sample analysis was carried out by an in-house accredited laboratory of Oil and Gas Production Division “Talakanneft” of “Surgutneftegas” PJSC (accreditation certificate No. ROSS RU.0001.517587 dated 31.10.2014) according to the approved methodology in compliance with the current directives and guidelines. Lower range of pollutant detection techniques does not exceed established standards for the safe content level (maximum allowable concentrations (MAC), approximate permissible concentration (APC), safe reference levels of impact (SRLI), etc).
The results of researches are submitted to authorized government bodies as hard copies before the 1st of April of the year following the reporting year.
Surface waters
In 2025, 134 samples of surface waters from six subsoil plots where LEM is performed were taken and examined. Samples were taken in a snowless period from June till September. 
The average concentration of hydrochemical indicators of LEM was calculated following the researches. Evaluation of the results of surface waters at subsoil plots is performed in compliance with the current specified parameters (MAC) established by Order No. 296 of Russian Federal Agency for Fishery “To approve the water quality standards for water bodies of fishery importance, including standards for maximum permissible concentrations of harmful substances in the waters of water bodies of fishery importance” dated 26.05.2025.
Table 2. Average concentration of hydrochemical indicators determined in surface waters in 2025
	Hydrochemical 
indicator
	Unit of measure
	Average value of hydrochemical indicators in 2025
	MAC1
	Ratio of average values to MAC

	pH value
	pH unit
	7.3
	-
	-

	Electrical
conductivity
	mmhos/cm
	133
	-
	-

	Ammonia and ammonium ions (in total)
	mg/dm3
	<0.1
	0.5 
	<0.2

	Nitrate ion
	mg/dm3
	<0.1
	40 
	<0.0025

	Biochemical oxygen demand (total BOD)
	mgО2/dm3
	2.2
	3.0
	0.74

	Phosphate ion
	mg/dm3
	<0.1
	0.2 
	<0.5

	Sulfate ion
	mg/dm3
	18.5
	100 
	0.19

	Chloride ion
	mg/dm3
	8.0
	300 
	0.03

	Anionic surfactants
	mg/dm3
	<0.025
	0.1
	<0.25

	Oil products
	mg/dm3
	<0.02
	0.05
	<0.4

	Volatile phenols
	mg/dm3
	<0.0005
	0.001 
	<0.5


	Iron
	mg/dm3
	0.22
	0.1 
	2.2

	Lead
	mg/dm3
	<0.003
	0.006 
	<0.5

	Zinc
	mg/dm3
	<0.005
	0.01 
	<0.5

	Nickel
	mg/dm3
	<0.005
	0.01 
	<0.5

	Manganese
	mg/dm3
	0.0137
	0.01
	1.37

	Chrome
	mg/dm3
	<0.002
	0.07 
0.02 
	<0.029
<0.1

	Copper
	mg/dm3
	0.0019
	0.001 
	1.9

	Mercury
	mcg/dm3
	<0.01
	0.01
	<1

	Suspended substance
	mg/dm3
	2.9
	-
	-

	toxicity level
	s.u.
	0.18
	-
	-


Water courses in the territory under study are located within the area of karst rocks. Water courses that disappear during the summer, the mismatch of watersheds of surface and underground waters are typical of karst regions. This results in an underground flowing of waters between river basins, the share of underground waters in the river recharge reaches 35-45%, the share of snow and rain recharge are approximately the same. In the winter period, the rivers are recharged solely by underground waters that are relieved into channel alluvial sediments. The natural state of rocks and soils in the territory forms geochemical specifics of surface watercourses in which almost widespread exceedance of the approved standards related to iron, manganese and copper is observed. 
Concentration of oil products and chlorides in surface waters, which characterizes the man-made pollutant flux in oil production regions, has special urgency when assessing the environmental situation in the region. In 2025, MAC exceedance of chlorides and oil products in surface waters was not identified.
Generally, the chemical composition of the analyzed water courses and water bodies is characterized by features common to the waters of the region.
Bottom sediments 
In 2025, 35 samples of bottom sediments were taken and analyzed at the subsoil plots where LEM was performed. The samples were taken once per year at sampling points of the surface water in summer.
There are no federal pollution standards set for the content of pollutants in the bottom sediments. 
For the reporting period, the total form of metals in the bottom sediments samples was taken into account. 
Table 3. Average values of determined indicators in bottom sediments when analyzing the background pollution level (2006 – 2012) and when performing LEM in 2025
	Indicator
	Unit of measure
	Average values
of determined indicators

	
	
	Background pollution level
(2006-2012)
	LEM
(2025)

	pH value
	pH unit
	6.8
	7.3

	Chlorides
	mg/kg
	19.9
	<10

	Sulfates
	mg/kg
	161
	23.8

	Oil products
	mg/kg
	69
	<50

	Iron (total content)
	mg/kg
	4933
	2621

	Lead (total content)
	mg/kg
	5.0
	6.2

	Zinc (total content)
	mg/kg
	76
	13.5

	Manganese (total content)
	mg/kg
	533
	144

	Chrome (total content)
	mg/kg
	16.1
	3.5

	Copper (total content)
	mg/kg
	8.8
	4.6

	Nickel (total content)
	mg/kg
	16.8
	1.9

	Specific electrical conductivity of the water extract
	mmhos/cm
	166
	103

	toxicity level
	s.u.
	0.20
	0.21


Current condition of bottom sediments of plots was assessed against the results of the measurement of the background pollution level performed, obtained in 2006-2012.
The average values of indicators determined in samples of bottom sediments taken in 2025 do not exceed the average values of the background pollution level determined in 2006-2012, except for total lead content.
Soils 
In 2025, 16 samples taken from subsoil plots where LEM was performed were analyzed as part of environmental monitoring.
Table 4. Average values of indicators determined in soils in 2025
	Indicator
	Unit of measure
	Average values of determined indicators
	MAC, APC1
	Ratio of average values to MAC

	pH of the water extract
	pH unit
	7.5
	-
	-

	Chlorides
	mg/kg
	7.1
	-
	-

	Sulphates
	mg/kg
	14.0
	-
	-

	Exchangeable ammonium
	mg/kg
	<5
	-
	-

	Nitrates
	mg/kg
	<1
	130.0
	0.01

	Phosphates
	mg/kg
	<1
	-
	-

	Oil products
	mg/kg
	<50
	-
	-

	Iron (total 
content)
	mg/kg
	3829
	-
	-

	Manganese (total content)
	mg/kg
	427
	1500
	0.29

	Zinc (total 
content)
	mg/kg
	65
	220
	0.3

	Lead (total 
content)
	mg/kg
	4.4
	130
	0.04

	Nickel (total 
content)
	mg/kg
	22
	80
	0.28

	Copper (total 
content)
	mg/kg
	10.0
	132
	0.08

	Chrome (total 
content)
	mg/kg
	10.1
	-
	-

	Iron (active form)
	mg/kg
	149
	-
	-

	Manganese (active form)
	mg/kg
	24
	60
	0.4

	Zinc (active form)
	mg/kg
	1.3
	23.0
	0.06

	Lead (active form)
	mg/kg
	<0.5
	6.0
	0.09

	Nickel (active form)
	mg/kg
	0.64
	4.0
	0.16

	Copper (active form)
	mg/kg
	0.73
	3.0
	0.25

	Chrome (active form)
	mg/kg
	0.38
	6.0 
	-

	Organic
substance
	mg/kg
	4.5
	-
	-

	Benz(o)pyrene
	mcg/kg
	<1
	20.0
	0.05

	Specific electrical conductivity of the water extract
	mmhos/cm
	60.6
	-
	-

	toxicity level
	s.u.
	0.20
	-
	-


The average values of determined indicators in soil samples taken as part of local environmental monitoring in 2025 do not exceed MAC and APC.
Ambient air
In 2025, 16 samples of ambient air from six subsoil plots were examined. These samples were taken at the subsoil plots where local environmental monitoring is performed. 
The samples were taken at six baseline monitoring points (least affected by a man and transboundary masses from technological facilities at the plots) and 10 control points (affected by man-made infrastructure facilities).
Five components were under research: methane, carbon monoxide, sulphur dioxide, nitrogen monoxide and nitrogen dioxide.
In accordance with environmental monitoring programs, the ambient air quality assessment was carried out on the basis of comparison of the results of the quantitative chemical analysis with MAC and SRLI standards. Levels exceeding hygienic standards were not determined.
Thus, the comprehensive analysis of the results of environmental monitoring within subsoil plots of “Surgutneftegas” PJSC for 2025 shows that the Company’s oil production facilities located within the Republic of Sakha (Yakutia) do not have a significant negative environmental impact. The overall characteristic of the environmental situation in the area where the Company operates is favorable. The impact of the Company’s production facilities is characterized as acceptable, i.e. it maintains the quality of the environment.


