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Summary report
on results of industrial environmental monitoring
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in 2025
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Industrial environmental monitoring (IEM) in “Surgutneftegas” PJSC is performed on the basis of GOST R 56059-2014 “Industrial environmental monitoring. General provisions” in order to provide information on the environment condition and pollution level required to perform activity on preservation and restoration of the natural environment, rational use and reproduction of natural resources, prevention of the negative impact of business, and other activity on the environment and elimination of its consequences.
According to GOST R 56059-2014, environmental analytical measurement can be performed only by in-house or third-party laboratories that are accredited for required measuring in compliance with the current legislation of the Russian Federation and have license to operate in the sphere of hydrometeorology and related areas.
“Surgutneftegas” PJCS holds license No. L039-00117-77/00299159 dated 17.06.2022 to operate in the sphere of hydrometeorology and related areas (with the exception of the specified activities carried out during engineering surveys conducted for the preparation of project documentation, construction, reconstruction of capital construction facilities), including determination of the pollution level of ambient air, soils and water bodies.
In the territory of Yamalo-Nenetsky Autonomous Okrug, environmental monitoring within subsoil plots is performed in compliance with Decree of the Government of YaNAO No. 56-p “On the territorial environmental monitoring system within license blocks for subsoil use for the purpose of oil and gas production in the territory of Yamalo-Nenetsky Autonomous Okrug” dated 14.02.2013.
“Surgutneftegas” PJSC holds six subsoil plots within Yamalo-Nenetsky Autonomous Okrug: Verkhne-Nadymsky (northern part) (SLKh 02565 NE), Vostochno-Soimlorsky (SLKh 02566 NR), Maloperevalny (SLKh 02573 NR), Severo-Soimlorsky (SLKh 02572 NR), Soimlorsky (SLKh 14822 NR), Tychelsky (SLKh 02574 NR). 
For the Verkhne-Nadymsky (northern part), Maloperevalny and Soimlorsky subsoil plots with constructed field infrastructure facilities, where commercial field operation is performed, programs on local environmental monitoring (hereinafter – LEM) are developed and approved in the established order.
At other plots, where field prospecting and exploration are carried out, industrial environmental monitoring is performed on the object-by-object basis as per project documentation and the current legislation in the sphere of industrial environmental monitoring on the basis of sampling schedules and schemes.
Thus, we performed environmental monitoring of three subsoil plots in the territory of YaNAO in 2025: the Verkhne-Nadymsky (northern part), Soimlorsky, and Maloperevalny.
The location for points of sampling natural environmental components is selected on the basis of the analysis of topographic maps, Earth remote sensing data taking into account hydrography and soil cover features of license blocks, as well as the location of production facilities. 
Natural environmental components under study: surface waters, soils, bottom sediments, snow cover (melted snow), and ambient air.
Table 1. The structure of the observational network of local environmental monitoring within subsoil plots of “Surgutneftegas” PJSC in the territory of YaNAO
	Natural environment components
	Points of monitoring status
	Number of points
	Number of controlled parameters

	Ambient air
	Conditional baseline 
	3
	8

	
	Conditional control 
	3
	8

	
	Control
	3
	8

	Snowfall
	Conditional baseline 
	3
	13

	
	Conditional control 
	3
	13

	
	Control
	3
	13

	Surface waters
	Conditional baseline 
	4
	18

	
	Conditional control
	6
	18

	
	Control
	4
	18

	Bottom sediments
	Conditional baseline 
	4
	12

	
	Conditional control
	6
	12

	
	Control
	4
	12

	Soils
	Conditional baseline 
	3
	20

	
	Conditional control
	3
	20

	
	Control
	3
	20


The laboratory sample analysis was carried out by two in-house accredited laboratories according to the approved methodology in compliance with the current regulations and guidelines:
1. Central Base Laboratory for Ecoanalytical and Technological Studies of the EEIC (accreditation certificate No. RA.RU.511426).
2. Production and Research Laboratory for chemical and physical analyses of R&D Design Works Center of OGPD “Nizhnesortymskneft” (accreditation certificate No. RA.RU.21CP03).
Lower range of pollutant detection techniques does not exceed established standards for the safe content level (maximum allowable concentrations (MAC), approximate permissible concentration (APC), safe reference levels of impact (SRLI), etc).
The results of the researches are submitted to authorized government bodies as hard and soft copies, and by means of information analytical system “Territorial system of environmental monitoring in YaNAO”.
Surface waters
In 2025, 28 samples of surface waters were examined. The samples were taken from the rivers Simiegan, Yangyagun, Mutiyagun, Tatlyagayakha, Lankiegan, an unnamed river, down the stream after crossing the communication line, and from lakes Yaeyakhato, Mutylor, an unnamed lake, Yangyaguntoilor. The results of the research (average values of core determined indicators) are shown in table 2.
Evaluation of the results of surface waters at the subsoil plots is performed in compliance with the current specified parameters (MAC) established by Order No. 552 of the Ministry of Agriculture of the Russian Federation dated 13.12.2016 and by Order No. 296 of Russian Federal Agency for Fishery dated 26.05.2025.
Table 2. The average values of hydrochemical indicators determined in surface waters in 2025 and MAC of controlled indicators in surface waters in the territory of YaNAO
	Hydrochemical 
indicator
	Unit of measure
	MAC
	Average value of hydrochemical indicators

	pH value
	pH unit
	-
	7.1

	BOD5
	mgО2/dm3
	2.1
	1.74

	Ammonium ion
	mg/dm3
	0.5
	0.15

	Nitrate ion
	mg/dm3
	40
	0.26

	Phosphate ion 
	mg/dm3
	0.2
	<0.1

	Sulfate ion
	mg/dm3
	100
	0.77

	Chloride ion
	mg/dm3
	300
	16.3

	Anionic surfactant 
	mg/dm3
	0.1
	<0.025

	Oil products
	mg/dm3
	0.050
	0.032

	Phenol
	mg/dm3
	0.001
	<0.0005

	Total iron
	mg/dm3
	0.1
	0.35

	Lead
	mg/dm3
	0.006
	0.0017

	Zinc
	mg/dm3
	0.01
	0.032

	Nickel
	mg/dm3
	0.01
	<0.005

	Manganese
	mg/dm3
	0.01
	0.035

	Copper
	mg/dm3
	0.001
	0.0020

	Hexavalent chrome
	mg/dm3
	0.02
	<0.01

	Mercury
	mg/dm3
	0.00001
	<0.00001


In 2025, the average concentration of all determined components did not exceed MAC, except for total iron, zinc, manganese and copper. 
Wetland water-collecting areas are the main source of iron, zinc, manganese and copper found in the surface waters of water courses. MAC exceedance of these elements is the key feature of the surface waters in the region. 
Concentration of oil products and chlorides in surface waters, which characterizes the man-made pollutant flux in oil production regions, has special urgency when assessing the environmental situation in the region. In 2025, MAC exceedance of chlorides and oil products in surface waters was not identified.
Generally, composition of the analyzed water courses and water bodies is characterized by features common to the taiga zone waters. Condition of surface waters was assessed as satisfactory.
Bottom sediments
In 2025, 14 bottom sediments samples were analyzed. The samples were taken once at sampling points of the surface water.
There are no federal pollution standards set for bottom sediments. The current bottom sediments condition of plots was assessed against the environmental quality standards (hereinafter – EQS) for bottom sediments established in the territory of YaNAO established by Order No. 3003 dated 08.09.2021 (table 3).
Table 3. The average values of indicators determined in bottom sediments in 2025 and EQS determined for bottom sediments in the territory of YaNAO
	Determined 
indicator
	Unit of measure
	Average value of indicator
	EQS indicators within Nadymsky District
	EQS indicators within Pur river basin

	pH
value (рН) of the water extract
	pH unit
	6.6
	6.15
	6.37

	Chloride ion
	mg/kg
	8.15
	32.49
	25.37

	Sulfate ion
	mg/kg
	23.8
	64.87
	66.03

	Anionic surfactant
	mg/kg
	6.41
	1.22
	1.64

	Oil products
	mg/kg
	<50
	4.85
	6.47

	Iron
	mg/kg
	212
	10699.6
	13561.7

	Lead
	mg/kg
	0.05
	4.27
	4.03

	Zinc
	mg/kg
	2.9
	18.47
	12.94

	Nickel
	mg/kg
	1.36
	11.64
	4.15

	Manganese
	mg/kg
	11.8
	141.97
	179.09

	Chrome VI
	mg/kg
	<0.05
	23.6
	10.56

	Copper
	mg/kg
	0.54
	4.08
	2.59


Bottom sediments are a comprehensive multicomponent system, the condition of which depends on intrabasin processes, sorption properties of sediments, landscape features of water courses, as well as properties of chemicals that make up their composition. Also, a significant impact is made by climatic factors, including the amount of precipitation and the level of floodwaters. The unstable composition and properties of bottom sediments is caused by the naturally-occurring environmental and climatic fluctuations.
There was no exceedance identified against EQS within YaNAO, except for anionic surfactants and oil products. The average concentration of anionic surfactant products exceeded the average regional values by 5.3 times in Nadymsky District and by 3.9 times in Purovsky District. It is important to note that the concentration of oil products in all samples taken in 2025 did not exceed the average values of oil products concentration (132 mg/kg), that were established during the assessment of the baseline condition of the bottom sediments at the Verkhne-Nadymsky (northern part), Soimlorsky and Maloperevalny subsoil plots of “Surgutneftegas” PJSC in YaNAO.
Soils
In 2025, 9 soil samples were analyzed as part of LEM. 
The current soil condition of subsoil plots in YaNAO was assessed against the approved soil standards (MAC, APC). The average values of the indicators determined in soils in 2025 are presented in table 4.
Table 4. The average values of indicators determined in soils in 2025.
	Determined 
indicator
	Unit of measure
	MAC, APC
	Average value of indicator
	Ratio of average values to MAC

	pH of the water extract
	pH unit
	-
	6.13
	-

	Phosphate ion
	mg/kg
	-
	<0.5
	-

	Nitrate ion
	mg/kg
	130
	1.44
	0.02

	Sulfate ion
	mg/kg
	-
	4.61
	-

	Chloride ion
	mg/kg
	-
	17.4
	-

	Oil products
	mg/kg
	-
	15.3
	-

	Anionic surfactant
	mg/kg
	-
	13.2
	-

	Phenol
	mg/kg
	-
	<0.010
	-

	Benz(o)pyrene
	mg/kg
	0.02
	<0.0002
	0.01

	Mercury
	mg/kg
	2.1
	<0.05
	0.03

	Hexavalent chrome
	mg/kg
	-
	<0.05
	-

	Iron
	mg/kg
	-
	1011
	-

	Copper
	mg/kg
	33
	2.55
	0.08

	Nickel
	mg/kg
	20
	<0.1
	0.01

	Zinc
	mg/kg
	55
	<5
	0.09

	Lead
	mg/kg
	32
	<0.1
	0.01

	Cadmium
	mg/kg
	0.5
	<0.05
	0.1

	Manganese
	mg/kg
	1500
	20.5
	0.02

	Barium
	mg/kg
	-
	<5
	-


Exceeding of MAC, APC in soil was not indicated. The average values of determined indicators in soil samples taken as part of LEM make up one and two decimal digits of established environmental standards.
The content of oil products in soil samples taken at the subsoil plots under development was 15.3 mg/kg on average, which coincides with a baseline content of oil products in the soil based on Yu.I.Pikovsky’s measurement scale (1993).
Snow cover (snow melt)
In 2025, 9 samples of the snow cover were examined at the said subsoil plots. Samples were taken during the period of maximum stored moisture (March) at three conditional baseline points (least affected by man), three conditional control points (affected by man-made infrastructure facilities), and three control points. Mean values of core indicators determined in snow cover during 2025 are presented in table 5.
Table 5. The average values of indicators determined in the snow cover (melted snow) in 2025 and EQS of indicators determined in the snow cover (melted snow) in the territory of YaNAO 
	Determined
indicator
	Unit of measure
	Average values 
of determined indicators
	EQS 
within Nadymsky District
	EQS 
within Purovsky District

	
	
	Conditional baseline points
	Conditional control points
	
	

	Ammonium ion
	mg/dm3
	0.10
	0.10
	0.27
	0.25

	Nitrate ion
	mg/dm3
	1.01
	0.19
	0.77
	0.92

	Sulfate ion
	mg/dm3
	1.53
	<0.1
	0.54
	0.37

	Chloride ion
	mg/dm3
	1.15
	0.97
	0.82
	0.58

	Oil products
	mg/dm3
	<0.06
	<0.06
	0.028
	0.033

	Phenol
	mg/dm3
	<0.0005
	<0.0005
	0.0008
	0.0006

	Total iron
	mg/dm3
	<0.050
	<0.050
	0.091
	0.071

	Lead
	mg/dm3
	0.0066
	0.0045
	0.0027
	0.0024

	Zinc
	mg/dm3
	0.04
	0.037
	0.0119
	0.0102

	Manganese
	mg/dm3
	0.0019
	0.0010
	0.0045
	0.0074

	Copper
	mg/dm3
	0.0038
	0.0034
	0.0026
	0.0025

	Nickel
	mg/dm3
	<0.0010
	<0.0010
	0.0019
	0.0028

	Hexavalent chrome
	mg/dm3
	<0.01
	<0.01
	0.0018
	0.0025


There are no federal environmental pollution standards set for snow cover. Snow cover quality appraisal was carried out on the basis of comparison of average values of the results of quantitative chemical analysis of samples taken at conditional baseline and conditional control monitoring points and of the environmental quality standards (EQS) for snow cover established in the territory of YaNAO. 
A slight concentration excess of nitrate ion, sulfate ion, copper, lead and zinc is present against EQS within YaNAO. 
The average concentration of the controlled indicators did not exceed values determined at conditional baseline points in 2025.
Ambient air
In 2025, 18 samples of ambient air were examined. The samples were taken at three conditional baseline monitoring points (least affected by man and transboundary masses from technological facilities at the plots), three conditional control points (affected by man-made infrastructure facilities), and three control points.
The content of methane, carbon monoxide, sulphur dioxide, nitrogen monoxide, nitrogen dioxide, suspended materials, carbon and benz(o)pyrene was determined.
Concentration of determined components in 2025 was below the low value of measurement ranges of methods for: methane <20 mg/cubic meters, carbon monoxide <4 mg/cubic meters, sulphur dioxide <0.054 mg/cubic meters, nitrogen monoxide <0.086 mg/cubic meters, nitrogen dioxide <0.086 mg/cubic meters, suspended materials (dust) <0.15 mg/cubic meters, carbon (carbon dust) <0.03 mg/cubic meters and benz(o)pyrene <0.5*10-6 mg/cubic meters.
The ambient air quality assessment was carried out on the basis of comparison of the results of the quantitative chemical analysis with MAC and SRLI standards. Levels exceeding hygienic standards were not determined. Pollution level of ambient air is within maximum allowable ranges and is considered “low”.
The area of operations of “Surgutneftegas” PJSC in YaNAO is not exposed to long and intensive exploitation of natural resources, which in turn translates into the low level of the human impact and burden on the environment.
The analysis of the results received during environmental monitoring of subsoil plots “Surgutneftegas” PJSC in YaNAO confirms that the general environmental situation in the area where the Company operates is favorable. The impact of the Company’s production facilities is characterized as acceptable, i.e. it maintains the quality of the environment.


