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Industrial environmental monitoring (IEM) in “Surgutneftegas” PJSC is performed in accordance with GOST R 56059-2014 “Industrial environmental monitoring. General provisions” to provide information on the environment condition and pollution level required to carry out activity on preservation and restoration of the natural environment, rational use and reproduction of natural resources, prevention of the negative impact of business and other operations on the environment and elimination of their consequences.
In 2024 the works were performed in accordance with license of “Surgutneftegas” PJSC No. L039-00117-77/00299159 dated 17.06.2022 to operate in the field of hydrometeorology and related fields (with the exception of the specified activities carried out during engineering surveys conducted for the preparation of project documentation, construction, reconstruction of capital construction facilities), including assessment of the pollution level of ambient air, soils and water bodies.
Industrial environmental monitoring at subsoil plots in the territory of Khanty-Mansiysky Autonomous Okrug – Yugra is performed in compliance with Decree of the Government of Khanty-Mansiysky Autonomous Okrug – Yugra No. 485-p dated 23.12.2011 “On environmental monitoring system within license blocks for subsoil use for the purpose of oil and gas production in the territory of Khanty-Mansiysky Autonomous Okrug – Yugra and annulment of some decrees of the Government of Khanty-Mansiysky Autonomous Okrug – Yugra”. 
The monitoring system is developed in compliance with projects of local environmental monitoring and projects for assessment of the initial contamination of natural environment components within subsoil plots of “Surgutneftegas” PJSC.
During the development of the monitoring system the regional features were taken into consideration, including: vast area of the territory, marshiness of the land, developed river net as well as the location of production facilities.
Monitoring points are installed at all major water bodies in the territory of the Company’s operations, at the prevailing types of soils as well as in the areas where main production facilities are located, i.e. places that pose potential environmental risks. 
In 2024, within subsoil plots of “Surgutneftegas” PJSC in KhMAO – Yugra the monitoring was performed at 62 subsoil plots, including local environmental monitoring (hereinafter – LEM) at 1084 sampling points at 61 subsoil plots, and baseline pollution assessment (hereinafter – BPA) at 19 sampling points at one subsoil plot. Monitoring points are fixed in the field by identification marks containing information about the number, geographical coordinates and name of the subsoil plot.
Natural environment components under study: surface waters, bottom sediments, soils, ambient air and snow cover.

The structure of the observational network of environmental monitoring within subsoil plots of “Surgutneftegas” PJSC in the territory of 
Khanty-Mansiysky Autonomous Okrug – Yugra
	Natural environment
components
	Type of monitoring
	Number of points
	Number of controlled parameters

	Ambient air
	BPA
	1
	7

	
	LEM
	186
	7

	Snowfall
	BPA
	1
	13

	
	LEM
	177
	13

	Surface waters
	BPA
	7
	22

	
	LEM
	268
	22

	Bottom sediments
	BPA
	7
	20

	
	LEM
	258
	14

	Soils
	BPA
	3
	23

	
	LEM
	195
	17



The laboratory sample analysis is carried out by seven in-house accredited laboratories according to approved methodology in compliance with the current regulations and guidelines. Lower range of pollutant detection techniques does not exceed established standards for the safe content level (maximum allowable concentrations (MAC), approximate permissible concentration (APC), safe reference levels of impact (SRLI), etc).
The research results are submitted to the Department for Environmental, Wildlife and Forestry Affairs Control of Khanty-Mansiysky Autonomous Okrug – Yugra (Prirodnadzor of Yugra) by means of web-service “Natural resources user profile” of information exchange system “Environmental passport of Khanty-Mansiysky Autonomous Okrug – Yugra” during the established period as well as in electronic form until the first day of April of the year following the reporting year.

Surface waters
In 2024, 762 samples of surface waters from 61 subsoil plots under LEM and 14 samples of surface waters from one subsoil plot under BPA, were taken and underwent a comprehensive chemical analysis. 
Evaluation of the results of BPA and LEM of surface waters at subsoil plots is performed against the current specified parameters (MAC), established by Order of the Ministry of Agriculture of the Russian Federation No. 552 dated 13.12.2016.

Average concentration of hydrochemical indicators
determined in surface waters 
	Hydrochemical indicator
	Unit
	Average value (AV)
 of hydrochemical indicators
	MAC
	AV to MAC ratio in 2024

	
	
	BPA 
	LEM 
	
	

	
	
	2023
	2024
	2023
	2024
	
	BPA
	LEM

	pH 
value
	pH unit
	7.2
	7.3
	7.2
	7.4
	n/a
	-
	-

	BOD, ultimate 
	mgО2/dm3
	2.8
	2.8
	2.8
	2.8
	3.0
	0.93
	0.93

	Ammonium ion
	mg/dm3
	0.19
	0.21
	0.21
	0.14
	0.5
	0.42
	0.28

	Nitrate ion
	mg/dm3
	0.53
	0.69
	0.68
	0.67
	40
	0.017
	0.017

	Phosphate ion
	mg/dm3
	<0.1
	<0.1
	<0.1
	<0.1
	0.2
	<0.5
	<0.5

	Sulfate ion
	mg/dm3
	0.15
	0.91
	1.12
	1.14
	100
	0.009
	0.011

	Chloride ion
	mg/dm3
	19
	17
	14
	13.7
	300
	0.06
	0.046

	Anionic surfactant
	mg/dm3
	<0.025
	<0.025
	<0.025
	<0.025
	0.1
	<0.25
	<0.25

	Oil products
	mg/dm3
	0.030
	0.027
	0.024
	0.026
	0.05
	0.54
	0.52

	Phenol
	mg/dm3
	<0.0005
	<0.0005
	<0.0005
	<0.0005
	0.001
	<0.005
	<0.005

	Total iron
	mg/dm3
	0.25
	0.8
	0.41
	0.47
	0.1
	8
	4.7

	Lead
	mg/dm3
	<0.003
	0.0034
	<0.003
	<0.003
	0.006
	0.68
	<0.5

	Zinc
	mg/dm3
	0.034
	0.0112
	0.031
	0.025
	0.01
	1.12
	2.5

	Nickel
	mg/dm3
	<0.005
	<0.005
	<0.005
	<0.005
	0.01
	<0.5
	<0.5

	Manganese
	mg/dm3
	0.021
	0.015
	0.049
	0.04
	0.01
	1.5
	4.0

	Hexavalent chrome 

	mg/dm3
	<0.01
	<0.01
	<0.01
	<0.01
	0.02
	<0.5
	<0.5

	Copper
	mg/dm3
	0.0047
	0.001
	0.002
	0.0016
	0.001
	1.0
	1.6

	Mercury
	mcg/dm3
	<0.01
	<0.01
	<0.01
	<0.01
	0.01
	<1
	<1



The landscape of the West Siberian taiga zone is featured by a large number of wetlands. The chemical composition of bog waters is characterized by high acidity. The acidic media of aquifers, formed due to a high level of marshiness is beneficial for the migration of micro- and macroelements. This determines a high concentration of iron, manganese, zinc and copper in the surface waters of the autonomous okrug. 
Natural landscape-geochemical conditions cause almost widespread exceedance of the approved standards related to iron (79% of samples taken at sites of BPA and 78% of samples taken at sites of LEM), manganese (64% of samples taken at sites of BPA and 63% of samples taken at sites of LEM), zinc (43% of samples taken at sites of BPA and 52% of samples taken at sites of LEM) and copper (43% of samples taken at sites of BPA and 39% of samples taken at sites of LEM).
Usually, a high water season on large Siberian rivers takes a long time from two to four months depending on dryness of the year. A long period of flooding of vast bottomland areas increases the impact of biology-and-soil factors on formation of the chemical compound of surface waters. This translates into increasing concentration of nitrogen, phenol compounds generated by decomposition of plant remains.
In 2024, the average value of the determined hydrochemical indicators of soil samples taken as part of LEM do not exceed the average values of indicators of samples taken in 2023. 
High concentration of pollutants, that shows contamination level, was not determined.
Concentration of oil products and chlorides in surface waters, which characterize the man-made pollutant flux in oil production regions, has special urgency when assessing the environmental situation in the region. In compliance with Decree of the Government of Khanty-Mansiysky Autonomous Okrug – Yugra No. 485-p dated 23.12.2011, surface waters sampling for concentration determination of oil products and chlorides as priority pollutants shall be performed at points of LEM on a monthly basis during free channel period with due account for hydrographic features of water bodies.
In 2024, MAC exceedance of chlorides and oil products in surface waters was not identified.

Bottom sediments 
In 2024, 258 samples of bottom sediments were taken and analyzed at 61 subsoil plots where LEM was conducted and 14 samples of bottom sediments were taken and analyzed at one subsoil plot under BPA. The samples were taken once per year at surface water sampling points.



Average values of determined bottom sediments indicators 
	Indicator
	Unit of measure
	Average values of determined indicators

	
	
	BPA
	LEM

	
	
	2023
	2024
	2023
	2024

	pH value
	pH unit
	6.48
	6.57
	6.40
	6.44

	Organic substance
	%
	0.72
	7.77
	4.98
	4.24

	Chloride ion
	mg/kg
	8.03
	4.17
	23.9
	9.5

	Sulfate ion
	mg/kg
	10.4
	9.8
	22.2
	9.9

	Oil products
	mg/kg
	<50
	<50
	<50
	<50

	Iron (active form)
	mg/kg
	26
	65.3
	107
	144

	Lead (active form)
	mg/kg
	<0.5
	<0.5
	<0.5
	<0.5

	Zinc (active form)
	mg/kg
	<1
	<1
	1.02
	<1

	Manganese (active form)
	mg/kg
	3.4
	4.4
	13.7
	11.7

	Copper (active form)
	mg/kg
	<0.4
	<0.4
	<0.4
	<0.4

	Nickel (active form) 
	mg/kg
	<0.4
	<0.4
	<0.4
	<0.4

	Hexavalent chrome 
	mg/kg
	<0.05
	<0.05
	<0.05
	<0.05

	Mercury
	mg/kg
	<0.05
	<0.05
	<0.05
	<0.05



There are no federal pollution standards set for the content of pollutants in bottom sediments. Current condition of bottom sediments was assessed against results of BPA measurement performed in 2024 and against results obtained in 2023.
The average values of all determined indicators of bottom sediments samples taken as part of LEM do not exceed the average values of indicators of samples taken in 2023.
Soils 
In 2024, as part of environmental monitoring, 195 soil samples were taken at 61 subsoil plots under LEM and three soil samples were taken at one subsoil plot under BPA.

Average values of indicators determined in soil
	Indicator
	Unit of measure
	Average value (AV) 
of determined indicators
	MAC 
	AV to MAC ratio in 2024

	
	
	BPA
	LEM
	
	

	
	
	2023
	2024
	2023
	2024
	
	BPA
	LEM

	рН of salt
 extract
	pH unit
	3.5
	3.2
	3.58
	3.82
	-
	-
	-

	Organic substance
	%
	1.06
	4.27
	4.12
	5.3
	-
	-
	-

	Ammonium ion
	mg/kg
	<0.5
	<0.5
	0.62
	1.03
	-
	-
	-

	Phosphate ion
	mg/kg
	<0.5
	<0.5
	<0.5
	0.6
	-
	-
	-

	Nitrate ion
	mg/kg
	2.1
	0.51
	2.03
	1.85
	130
	0.004
	0.014

	Sulfate ion
	mg/kg
	6.8
	8.3
	9.99
	7.49
	-
	-
	-

	Chloride ion
	mg/kg
	4.25
	3.7
	5.9
	7.34
	-
	-
	-

	Oil products
	mg/kg
	12.3
	18
	15
	10.15
	-
	-
	-

	Benz(o)pyrene
	mg/kg
	0.00023
	<0.0002
	0.00026
	<0.0002
	0.02
	0.01
	0.01

	Iron 
(active form)
	mg/kg
	24.5
	87.7
	36.7
	65.9
	-
	-
	-

	Lead 
(active form)
	mg/kg
	<0.5
	<0.5
	<0.5
	<0.5
	6.0
	0.083
	0.083

	Zinc
(active form)
	mg/kg
	1.87
	<1.0
	<1.0
	<1.0
	23
	0.05
	0.05

	Manganese
(active form)
	mg/kg
	5.2
	<5
	5.32
	<5
	100
	0.05
	0.05

	Copper
(active form)
	mg/kg
	<0.4
	<0.4
	<0.4
	<0.4
	3.0
	0.13
	0.13

	Nickel 
(active form)
	mg/kg
	<0.4
	<0.4
	<0.4
	<0.4
	4.0
	0.1
	0.1

	Hexavalent chrome
	mg/kg
	<0.05
	<0.05
	<0.05
	<0.05
	-
	-
	-



The average values of determined indicators of soil samples taken as part of LEM do not exceed the average values of indicators of samples taken in 2023. Such values make up one and two decimal digits of the established environmental standards.
The content of oil products in soil samples taken at plots under development was 10.15 mg/kg on average, which coincides with the baseline content of oil products in the soil based on Pikovsky’s measurement scale (1993). 
Ambient air
In 2024, 372 samples of ambient air from 61 subsoil plots were examined. These samples were taken at the subsoil plots under LEM. The samples were taken at 62 baseline monitoring points (least affected by a man and transboundary masses from technological facilities at the plots) and 124 control points (affected by man-made infrastructure facilities). Also, two samples of air were taken and analyzed at one subsoil plot under BPA.
Seven components were under research: methane, carbon monoxide, sulphur dioxide, nitrogen oxide and dioxide, suspended materials, carbon black. 
In accordance with LEM projects, ambient air quality assessment was carried out on the basis of comparison of the results of quantitative chemical analysis with MAC and SRLI standards. Levels exceeding hygienic standards were not determined.
Monitoring results prove that ambient air condition was favorable in 2024. 

Snow cover (snow melt)
In 2024, 177 samples of snow cover from 60 subsoil plots under LEM were examined. The samples were taken during the period of maximum stored moisture (March–April) at 62 baseline monitoring points (not affected by the man-made impact) and 115 control points. Also, one sample of snow was taken and analyzed at one subsoil plot under BPA.



[bookmark: _GoBack]Average values of determined indicators
in snow cover (snow melt) 
	Determined 
indicator
	Unit of 
measure
	Average values
of determined indicators
	Average regional values (ARV)

	
	
	Baseline points
	Control points
	

	
	
	2023
	2024
	2023
	2024
	

	pH value
	pH unit
	5.2
	5.2
	5.1
	5.2
	5.6

	Ammonium ion
	mg/dm3
	0.067
	0.15
	0.069
	0.11
	0.24

	Nitrate ion
	mg/dm3
	1.25
	0.58
	1.26
	0.61
	1.04

	Sulfate ion
	mg/dm3
	1.4
	0.58
	1.34
	0.58
	1.48

	Chloride ion
	mg/dm3
	0.96
	0.53
	0.95
	0.57
	1.63

	Oil products 
	mg/dm3
	<0.020
	<0.06
	<0.020
	<0.06
	0.046

	Phenol
	mg/dm3
	0.00072
	<0.0005
	0.00051
	<0.0005
	0.0026

	Total iron
	mg/dm3
	<0.05
	<0.05
	<0.05
	<0.05
	0.07

	Lead
	mg/dm3
	0.0019
	0.0021
	0.0019
	0.0021
	0.0051

	Zinc
	mg/dm3
	0.053
	0.019
	0.042
	0.002
	0.019

	Manganese
	mg/dm3
	0.0014
	0.001
	0.001
	<0.001
	0.018

	Nickel
	mg/dm3
	<0.001
	<0.001
	<0.001
	<0.001
	0.0028

	Chrome (VI)
	mg/dm3
	<0.01
	<0.01
	<0.01
	<0.01
	0.008



There are no environmental standards set for snow cover. Snow cover quality appraisal was carried out on the basis of comparison of the average values of the results of quantitative chemical analysis of samples taken at monitoring checkpoints and points that are not affected by the man-made impact (baseline) as well as of the average regional values (ARV) obtained through the monitoring of snow cover in the territory of the autonomous okrug in the period of 2009–2019, and average values of 2023. 
Against the results obtained in the previous year, in 2024 the average concentration of all controlled indicators in the snow samples taken at the control points does not exceed the values determined at baseline points and values set in 2023. 
The average values of determined indicators in the snow samples taken at the control and baseline points do not exceed ARV.

Thus, the comprehensive analysis of the results of environmental monitoring within subsoil plots of “Surgutneftegas” PJSC for 2024 shows that the Company’s oil production facilities located within Khanty-Mansiysky Autonomous Okrug – Yugra, do not have a significant negative environmental impact. The overall characteristic of the environmental situation in the area where the Company operates is favorable. 
The impact of the Company’s production facilities is characterized as acceptable, i.e. ensuring compliance with environmental quality standards.
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